{"text_format":"1","workbook":"xlsx","n_sheets":7,"sheets":["Cover","Form A","Form B","Form C","Form D","Form E","W-9"],"not_rendered":{"charts":0,"images":13,"macros":1,"external_links":0,"defined_names":22,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Cover","index":0,"n_rows":17,"n_cols":4,"rows_kept":17,"cut":false,"hidden":false,"merged":[[1,3,1,5],[1,1,1,2],[2,1,2,5],[15,1,15,5],[16,1,16,5],[4,2,4,5]]}
[]
[null,null,null,"SECTION-C: H-GAC FORMS"]
[null,"For Use In Responding To Competitive Bid And Proposal Invitations"]
[null,"Invitation No.:","SW04-16"]
[null,"Title:","Sweeping Equipment"]
[]
[null,"This Section contains the following H-GAC Forms."]
[null,null,"FORM","DESCRIPTION"]
[null,null,"Form A:","Offeror Identification and Authorized Signatory"]
[null,null,"Form B:","Historically Underutilized Business Enterprises"]
[null,null,"Form C:","Response Checklist"]
[null,null,"Form D:","Offered Items Pricing"]
[null,null,"Form E:","Published Options"]
[null,null,"W-9","Reference attached document"]
[]
[null,"These forms are hereby made available in electronic format. They should be copied to Offeror's computer for completion and/or printout as required.  The forms may not be changed or altered in any way, except as may be specified on the form."]
[null,"All completed forms must also be submitted in printed media, as well as electronically, on CD-ROM, flash drive, etc., excepting of course for signatures. The printed \"Original\" of the response will be considered as the official copy in case of any discrepancy between the electronic version and the printed Original."]

{"sheet":"Form A","index":1,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[[26,2,26,8],[30,1,30,9],[31,7,31,9],[32,2,32,5],[32,7,32,9],[25,2,25,4],[25,6,25,8],[8,2,8,9],[10,2,10,9],[12,2,12,4],[12,6,12,8],[13,2,13,8],[14,2,14,3],[14,6,14,9],[19,0,19,10],[20,2,20,5],[20,7,20,9],[21,2,21,9],[23,2,23,9],[0,0,0,6],[1,2,1,9],[3,2,3,9],[4,2,4,9],[7,2,7,5],[7,7,7,9],[0,7,0,9]]}
["  FORM-A: OFFEROR IDENTIFICATION & AUTHORIZED SIGNATORY\n(DO NOT handwrite this form.  Information must be typed in.)",null,null,null,null,null,null,"Invitation #: SW04-16"]
[null,"Invitation Title:","Sweeping Equipment"]
[]
[null,"Offeror Company:"]
[null,null,"(Legal name of business which will appear on contract, if awarded)"]
[null,"Offeror Status:"]
[null,"Response Type (1):"]
[null,"Contract Signatory (2):",null,null,null,null,"Title:"]
[null,"Mailing Address (3):"]
[null,null,"Street/PO Box",null,null,null,"City",null,"State & Zip"]
[null,"Physical Address:"]
[null,null,"Street",null,null,null,"City",null,"State & Zip"]
[null,"Phone:",null,null,null,"Fax:"]
[null,"Email Address:"]
[null,"Federal Tax ID No.:",null,null,null,"Web Page URL:"]
[null,"     (1) If Joint Offering, all parties must submit a signed Form A.  A contract will be offered to each."]
[null,"     (2) Person who will sign final contract documents if an award is made."]
[null,"     (3) Address to which final contract documents would be sent for signature."]
[]
["Member Contact Information"]
[null,"Contact Person (4):",null,null,null,null,"Title:"]
[null,"Mailing Address:"]
[null,null,"Street/PO Box",null,null,null,"City",null,"State & Zip"]
[null,"Physical Address:"]
[null,null,"Street",null,null,null,"City",null,"State & Zip"]
[null,"Toll Free Phone:",null,null,null,"Fax:"]
[null,"Email Address:"]
[null,"     (4) Person who End Users will contact for product information and to get pricing quotes."]
[]
[null,"The Signatory below, on behalf of Offeror:"]
[null,"- Acknowledges having thoroughly reviewed the Invitation;\n- Attests to having the authority to sign this response and commit Offeror to honor all requirements;\n- Makes, under penalty of perjury, all required Offeror Certifications as detailed in General Terms;\n- Certifies that all information provided in this Response is true and correct."]
[null,"Required Signature:",null,null,null,null,"Title:"]
[null,"Printed Name:",null,null,null,null,"Date:"]

{"sheet":"Form B","index":2,"n_rows":19,"n_cols":9,"rows_kept":19,"cut":false,"hidden":false,"merged":[[0,0,0,7],[8,0,8,9],[5,0,5,9],[6,0,6,9],[4,0,4,9],[7,0,7,9],[1,1,1,9],[2,1,2,9],[0,8,0,9],[20,0,20,9],[10,0,10,9],[11,1,11,7],[18,0,18,9],[13,0,13,9],[14,0,14,9],[15,0,15,9],[16,0,16,9],[17,0,17,9]]}
["  FORM-B: HISTORICALLY UNDERUTILIZED BUSINESS ENTERPRISES",null,null,null,null,null,null,null,"Invitation #: SW04-16"]
["Title:","Sweeping Equipment"]
["Offeror:"]
[]
["Most, if not all, of the Members of HGACBuy are subject to various requirements relative to purchasing goods and services from Historically Underutilized Business Enterprises (HUBs)(See Note 1).  These requirements are promulgated by federal and state governmental authorities, and include measureable criteria such as 'percentage of total dollars spent directed to HUBs', 'number of HUB contractors used', 'HUB subcontractors employed by primary contractors', etc.  These requirements are generally formalized in goal oriented programs."]
["HGACBuy is comitted to promoting full and equal business opportunities for HUB contractors, and to assisting Cooperative Purchasing Program (COOP) Members in meeting mandated HUB goals.  In that regard, Contractor shall make a good faith effort to use the services of Certified/Listed (See Note 2) HUBs whenever possible."]
["As part of a good faith effort, Contractor agrees to work with and assist HGACBuy Members in meeting HUB targets and goals, as may be required by any rules, processes or programs they might have in place.  Such assistance may include such things as compliance with reporting requirements, provision of documentation, consideration of 'Certified/Listed' subcontractors, provision of documented evidence that an active participatory role for a HUB entity was considered in a procurement transaction, etc."]
["Note 1:  There are many designations other than \"HUB\" used across the country within various jurisdictions.  Examples include terms such as Disadvantaged Business Enterprise (DBE), Minority Owned Business Enterprise (MBE), Woman Owned Business Enterprise (WBE), Small Disadvantaged Business (SDB), Small, Woman or Minority-owned Business (SWAM), etc.  Regardless of the formal designation, the overall objective of the relavant programs is basically the same, i.e. to insure that disadvantaged and underutilized members of the business community receive a fair share of public spending.  The term HUB as used herein shall be understood to encompass all such programs/business enterprises, no matter what terminology is used by the Member."]
["Note 2:  The terms \"Certified\" and \"Listed\" as used in conjunction with HUB programs relate to the process of HUB qualification review.  Jurisdictions usually require that companies claiming HUB status be reviewed and confirmed as meeting certain minimum requirements to claim that status, and that the review and confirmation process be carried out by certain designated entities.  They are then \"Certified\" or \"Listed\" by having their name included on an official listing published by the Certifying or Listing Authority."]
[]
["Accepted and Agreed By:"]
["Title:  ",null,null,null,null,null,null,null,"Date:  "]
[]
["HUB Status Of Offeror"]
[]
["Designation(s): "]
["Certifying/Listing Authority(s): "]
["Subcontracts"]
["On a separate sheet, list any subcontractors that would be employed in providing products or services related to this procurement.  Include subcontractor name, designation (HUB, DBE, etc.) and certifying/listing authority.\n"]

{"sheet":"Form C","index":3,"n_rows":14,"n_cols":10,"rows_kept":14,"cut":false,"hidden":false,"merged":[[0,8,0,9],[0,0,0,7],[6,1,6,8],[7,1,7,8],[8,1,8,8],[1,2,1,9],[2,2,2,9],[3,0,3,9],[1,0,1,1],[2,0,2,1],[13,1,13,8],[4,0,4,8],[12,1,12,8],[10,1,10,8],[11,1,11,8],[9,1,9,8],[5,1,5,8]]}
["  FORM-C:  RESPONSE CHECKLIST",null,null,null,null,null,null,null,"Invitation #: SW04-16"]
["Title:",null,"Sweeping Equipment"]
["Offeror:"]
["This form is provided to help insure that all required Response elements have been completed and included, or certified as being available upon request.  Responses that do not comply with all requirements may be considered non-compliant.  Offeror's signatory should review each item below to verify they have been addressed as per the bid specification."]
["This Response Includes:",null,null,null,null,null,null,null,null,"Initial"]
[1,"An \"Original\" of all required H-GAC forms and documents, plus one copy, each in a separate hard-sided 3-ring binder."]
["2","Comprehensive list of body options pricing on Form-E. "]
["3","A completed electronic copy of ALL Forms and any other bid response documents"]
["4","Detailed specification / quote sheet for for each Form-D model priced reflecting all standard components."]
["5","The required list of references."]
["6","A complete description of Offeror's \"service organization\" (Ref. Section-A)"]
["7","Complete warranty documentation for all Products offered."]
["8","Form CIQ, if required by law, completed and signed. Offeror should refer to webpage, www.ethics.state.tx.us/whatsnew/conflict_forms.htm to get instructions and download the Form."]
["9","Completed W-9 document"]

{"sheet":"Form D","index":4,"n_rows":152,"n_cols":4,"rows_kept":152,"cut":false,"hidden":false,"merged":[[0,0,0,2],[136,0,136,3],[73,0,73,3],[109,0,109,3],[1,0,1,1],[1,2,1,3],[2,0,2,3],[4,0,4,3],[13,0,13,3],[79,0,79,3]]}
["FORM-D: Base Unit Offered Prices    Reflecting 11-11-15 Addendum                                                                              Invitation No.:                                                                              ",null,null,"SW04-16"]
["Offeror Name:"]
["Note:  Offeror shall not modify this form in any way other than inputting company name and pricing.  All products listed below are to be considered as Base Units for purposes of this Invitation and any subsequent contract. Offeror shall determine which models to bid and fill in the H-GAC bid price in the appropriate cell. Additionally, Offeror shall bid a compressive list of manufacturer options (and if a normally a component, cab-chassis) on Form-E.  Unless shown otherwise on this or any other H-GAC specification document, all models shall be priced herein to include the manufacturer standard components and be functional sweepers as priced (less chassis on commercial chassis-mounted designs). NOTE: All sweeper bodies designed for mounting on commercial cab-chassis shall be priced on this form as inclusive of mounting costs, but exclusive of cab-chassis.  By submittal of pricing on this form, Offeror attests to this. Offeror shall refer to Section-B for more details."]
["H-GAC Product\nCode","Manufacturer","Base Unit Model & Description                                                                                                           ","Offered Price, in Whole Dollars"]
["A: Street Sweepers: Purpose Built/Custom Chassis"]
["AA01","Elgin","Pelican-NP: 3-wheel mechanical sweeper; engine: Deere 4045T diesel, 74 hp (EPA tier 4f); hopper: 3.5 cu. yds; water tank: 220 gallons; standard sweep path, max: 120\""]
["AA02","Elgin","Pelican-NR: 3-wheel mechanical waterless sweeper; engine: Deere 4045T diesel, 74 hp (EPA tier 4f); hopper: 3.5 cu. yds variable height dump; standard sweep path, max: 120\"; dust control skirts, dust extraction fan, filtered air exhaust."]
["AB01","Global Sweeping","M3: 3-wheel mechanical sweeper; center-forward cab; REAR DUMP; engine: Deere 4045D diesel, 115 hp; hopper: 5.6 cu yds; water tank: 220 gallons;  standard path, max: 125\" "]
["AB02","Global Sweeping","M4HSD: 4-wheel mechanical sweeper; Center Steer; RH or LH Dump; engine: Cummins ISB 280, hopper: 5.0 cu yds; water tank: 280 gallons;  standard path, max: 125\" "]
["AB03","Global Sweeping","M4: 4-wheel mechanical sweeper; center-forward cab; REAR DUMP; engine: Cummins diesel, 280 hp; hopper: 5.6 cu yds; water tank: 250 gallons;  standard path, max: 125\" "]
["AB04","Global Sweeping","M4 Electric Hybrid: 4-wheel mechanical sweeper; center-forward cab; engine: Cummins diesel with generator-lithium ion battery system; hopper: 5.6 cu yds; water tank: 250 gallons;  standard path, max:125\" "]
["AB05","Global Sweeping","R3: 3-wheel regenerative air Sweeper; center foreard cab; engine: Isuzu Tier IV Final 180HP, hopper: 6 cu. Yds; water tank: 230 gallons; standard path: 125\" "]
["AC01","Johnston","C201: 4-wheel compact vacuum sweeper; VMI diesel, 84 hp; hopper: 2.3 cu yds; water tank: 66 gallons; standard path, max:120\" "]
["B: Street Sweepers: Commercial Cab-Chassis Mount Design "]
["BA01","Elgin","Eagle F: mechanical broom sweeper; auxiliary engine: Cummins diesel, 74 hp (EPA tier 4f); hopper: 4.5 cu. Yds; variable height dump; water tank: 280 gallons; standard sweep path, max: 120\""]
["BA02","Elgin","Eagle FW: mechanical broom waterless sweeper; auxiliary engine: Deere 4045T diesel, 74 hp (EPA tier 4f); hopper: 4.5 cu. Yds; variable height dump; standard sweep path, max: 120\"; dust control skirts, dust extraction fan, filtered air exhaust"]
["BA03","Elgin","Eagle F-CNG: mechanical broom sweeper; auxiliary engine: GM 3.0L, 68 hp; hopper: 4.5 cu. yds variable height dump; water tank: 280 gallons; standard sweep path, max: 120\""]
["BA04","Elgin","Broom Badger: mechanical sweeper; auxiliary engine Kubota 59 hp diesel (EPA tier 4f); hopper: 4 cubic yards; variable height dump; water tank: 220 gallons; standard sweep path, max 114\""]
["BA05","Elgin","Broom Bear: mechanical sweeper; single diesel chassis-engine design; hopper: 4.5 cu. yds variable height dump, water tank: 350 gallons; standard sweep path, max: 144\""]
["BA06","Elgin","Road Wizard: mechanical sweeper; auxiliary engine: Cummins, 74 hp (EPA tier 4f); hopper: 5.4 cu. yds variable height dump; water tank: 340 gallons tank; standard sweep path, max: 120\""]
["BA07","Elgin","Whirlwind: vacuum air sweeper; auxiliary engine: Deere 4045T diesel, 74 hp (EPA Tier 4f) shared power design; hopper: 8 cu. yds.; water tank: 335 gallons; rear ground level dump; standard sweep path, max: 144\""]
["BA08","Elgin","Megawind: vacuum air sweeper, auxiliary engine: Deere JD4045T diesel, 115 hp (EPA Tier 3); hopper: 10 cu. yds, rear ground-level dump; water tank: 335 gallons; standard sweep path, max: 144”"]
["BA09","Elgin","Crosswind J: regenerative air sweeper; auxiliary engine Deere 4045T diesel (EPA Tier 4f); shared power design; hopper: 8 cu. yds; water tank: 240 gallons; standard sweep path, max: 144\""]
["BA10","Elgin","Crosswind J-CNG: regenerative air sweeper; auxiliary engine: GM 5.7L, 124 hp; hopper: 8 cu. yds; water tank: 240 gallons; standard sweep path, max: 144\""]
["BB01","Global Sweeping","Viajet 6: Recirculating Air Sweeper; auxiliary engine: Volkswagon, 74 HP; hopper: 8 cu. Yds: water tank: 500 gallons; dual gutter broom configuration; standard sweep path, max: 120\""]
["BC01","Gradall","Vacall -Vacuum Sweeper -AS10: vacuum Sweeper, single (chassis) engine design; hopper: 10 cu yds; water tank: 350-gallons; single broom configuration; standard sweep path max: 77\""]
["BC02","Gradall","Vacall -Vacuum Sweeper -AS10D: vacuum sweeper, single (chassis) engine design; hopper: 10 cu yds; water tank: 350-gallons; dual broom configuration; standard sweep path, max: 154\""]
["BC03","Gradall","Vacall - Vacuum Sweeper - AS13: Vacuum Sweeper, single (chassis) engine design; hopper: 13 cu yds; water tank: 350-gallons; single broom configuration; standard sweep path, max: 77\""]
["BC04","Gradall","Vacall - Vacuum Sweeper - AS13D: vacuum sweeper, single (chassis) engine design; hopper: 13 cu yds; water tank: 350-gallons; dual broom configuration; standard sweep path, max: 154\""]
["BC05","Gradall","Vacall - Vacuum Sweeper - AS16: vacuum sweeper, single (chassis) engine design; hopper: 16 cu yds; water tank: 350-gallons; single broom configuration; standard sweep path, max: 77\""]
["BC06","Gradall","Vacall - Vacuum Sweeper - AS16D: vacuum sweeper, single (chassis) engine design; hopper: 16 cu yds; water tank: 350-gallons; dual broom configuration;  standard sweep path, max: 154\""]
["BC07","Gradall","Vacall - All Catch AC10: vacuum, catch basin cleaner; single (chassis) engine design; hopper: 10 cu yds; water tank: 350-gallons"]
["BC08","Gradall","Vacall - All Catch AC13: vacuum, catch basin cleaner; single (chassis) engine design; hopper: 13 cu yds; water tank: 350-gallons."]
["BC09","Gradall","Vacall - All Catch AC16: vacuum, catch basin cleaner; single (chassis) engine design; hopper: 16 cu yds; water tank 350-gallons"]
["BD01","Johnston","ES 351: mechanical sweeper; single diesel chassis-engine design; hopper: 4.5 cu. yds variable height dump, water tank: 360 gallons; standard sweep path, max: 144\""]
["BD02","Johnston","VT651: vacuum sweeper; dual engine design; auxiliary engine: Deere 4045TF diesel, 84 hp; hopper: 8.5 cu yds; water tank: 415 gallons; dual steering; standard sweep path, max: 144\""]
["BD03","Johnston","VS651: vacuum sweeper; single engine design; gearbox auxiliary drive hydraulic drive system; hopper: 8.5 cu yds; water tank: 415 gallons; dual steering; standard sweep path, max: 144\""]
["BD04","Johnston","VT801: vacuum sweeper; dual engine design; auxiliary engine: Deere 4045H diesel, 115 hp; hopper: 10.8 cu yds; water tank: 535 gallons; dual steering; standard sweep path, max: 144\""]
["BD05","Johnston","RT655: regenerative air sweeper; dual engine design; auxiliary engine: Deere 4045HF diesel, 115 hp; hopper: 8.5 cu yds; water tank: 250 gallons; dual steering; standard sweep path, max: 144\""]
["BE01","Nite-Hawk","Raptor: vacuum sweeper; single engine-PTO-hydraulic pump design; water tank: 100 gallons; standard sweep path, max: 81”  (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["BE02","Nite-Hawk","Raptor Edge: vacuum sweeper; single engine-PTO-hydraulic pump design; water tank: 100 gallons; standard sweep path, max: 81” (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["BE03","Nite-Hawk","Raptor EcoMax: vacuum sweeper; single engine-PTO-hydraulic pump design; water tank: 100 gallons; standard sweep path, max: 81” (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["BE04","Nite-Hawk","Raptor Edge HD CNG: vaccum sweeper, single engine - PTO-hydraulic pump design, water tank: 100 gallons, standard sweeping path, max 81\" (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["BF01","Schwarze","A4 Storm: regenerative air sweeper; auxiliary engine: Yanmar 4TN98C Tier IV Final diesel, 68 hp; hopper: 4.5 cu. yds.; water tank: 130 gallons; standard sweep path, max: 120”"]
["BF02","Schwarze","A7 Tornado: regenerative air sweeper; auxiliary engine: Deere 4045T diesel, 115 hp; hopper: 8.4 cu. yds.; water tank: 250 gallons; standard sweep path, max: 144”"]
["BF03","Schwarze","A8 Twister: regenerative air sweeper; auxiliary engine: Deere 4045T Tier IV Final diesel, 115 hp; hopper: 6.0 cu. yds., high dump; water tank: 250 gallons; standard sweep path, max: 144\""]
["BF04","Schwarze","A9 Monsoon: regenerative air sweeper; auxiliary engine: Deere 4045HF275 Tier IV Final diesel, 140 hp; hopper: 9.6 cu. yds.; water tank: 250 gallons; standard sweep path, max: 144”"]
["BF05","Schwarze","M6 Avalanche SE: mechanical broom sweeper; single chassis-engine design; hopper: 5 cu. yds.; water tank: 350 gallons; standard sweep path, max: 134” "]
["BF06","Schwarze","M6 AvalancheTE: mechanical broom sweeper; dual engine design; auxiliary engine: Yanmar Tier IV Final  diesel, 68 Hp; hopper: 5 cu. yd; water tank: 200 gallons; standard sweep path, max: 134” "]
["BF07","Schwarze","GS6 Tempest: regenerative air sweeper; auxiliary engine: Deere 4045T Tier IV Final  diesel, 115 hp; Hopper: 6.5 cu. yds; water tank: 250 gallons, standard sweep path, max: 134”"]
["BF08","Schwarze","Updraft: regenerative air sweeper (conventional, small truck chassis-mounting); auxiliary engine: Kohler, 31 Hp;  hopper: 2 cu. yds.; water tank: 12 gallons; standard sweep path, max: 97\" "]
["BF09","Schwarze","Vortex: regenerative air sweeper; twin-engine design; cab-over application; hopper: 4.5 cu. yds.; water tank: 93 gallons; standard sweep path, max: 95\""]
["BF10","Schwarze","Gale Force: regenerative air sweeper; dual engine design; cab-over application; auxiliary engine:  Perkins, 51 hp diesel; hopper: 4.5 cu. yds; water tank: 93 gallons; standard sweep path, max: 103\" "]
["BG01","Stewart-Amos","Starfire S-4: mechanical broom sweeper; dual engine design; auxiliary engine: Kubota, 59 hp diesel; hopper: 4.0 cu. yds.; water tank: 200 gallons; standard sweep path, max: 120”; left hand steer/sweep; rear-right camera  "]
["BG02","Stewart-Amos","Starfire S-4XL: mechanical broom sweeper; dual engine design; auxiliary engine: Kubota, 59 hp diesel; hopper: 4.5 cu. yds.; water tank: 330 gallons; standard sweep path, max: 120”; left hand steer/sweep; rear-right camera  "]
["BG03","Stewart-Amos","Starfire S-5s: mechanical broom sweeper; single chassis-engine design; hopper: 5.0 cu. yds.; water tank: 350 gallons; standard sweep path, max: 120”; left hand steer/sweep; rear-right camera  "]
["BG04","Stewart-Amos","Starfire S-5t: mechanical broom sweeper; dual engine design; auxiliary engine: Kubota, 59 hp diesel; hopper: 5.0 cu. yds.; water tank: 350 gallons; standard sweep path, max: 120”; left hand steer/sweep; rear-right camera  "]
["BG05","Stewart-Amos","Starfire S-6s: mechanical broom sweeper; single chassis-engine design; hopper: 6.0 cu. yds.; water tank: 350 gallons; standard sweep path, max: 120”; left hand steer/sweep; rear-right camera  "]
["BG06","Stewart-Amos","Starfire S-6t: mechanical broom sweeper; dual engine design; auxiliary engine: Kubota, 59 hp diesel; hopper: 6.0 cu. yds.; water tank: 350 gallons; standard sweep path, max: 120”; left hand steer/sweep; rear/right-camera  "]
["BG07","Stewart-Amos","Galaxy R-4: mid-sized regenerative air sweeper; auxiliary engine: Kubota, 74 hp diesel; hopper: 4.6 cu. yds.; water tank: 130 gallons; standard sweep path, max: 120\"; left hand steer/sweep; rear/right-camera"]
["BG08","Stewart-Amos","Galaxy R-6: mid-sized regenerative air sweeper; auxiliary engine: Kubota, 74 hp diesel; hopper: 6.1 cu. yds.; water tank: 200 gallons; standard sweep path, max: 120\"; left hand steer/sweep; rear/right-camera"]
["BG09","Stewart-Amos","Galaxy R-6XL: regenerative air sweeper; auxiliary engine: Kubota, 74 hp diesel; hopper: 6.1 cu. yds.; water tank: 330 gallons; standard sweep path, max: 120\"; left hand steer/sweep; rear-right camera"]
["BI01","Tymco","210-D: regenerative air sweeper; auxiliary engine: Kubota V2403MT Tier 4i turbocharged diesel, 56 hp; hopper: 2.4 cu.yds.; standard sweep path, max: 98”"]
["BI02","Tymco","210h: regenerative air sweeper; Hdrive hydraulic power system; single engine design; BlueLogic Control System; hopper: 2.4 cu.yds.; standard sweep path, max: 98”"]
["BI03","Tymco","435: mid-sized regenerative air sweeper; auxiliary engine: Kubota V2403T  Tier 4i turbocharged diesel, 56 hp; hopper: 4 cu. yds.; water tank: 150 gallons; standard sweep path, max: 130\""]
["BI04","Tymco","DST-4: mid-sized regenerative air dustless sweeping technology sweeper; auxiliary engine: Kubota V2403T Tier 4i turbocharged diesel, 56 hp; hopper: 4 cu. yds.; water tank: 76 gallons; standard sweep path, max: 130”"]
["BI05","Tymco","DST-6: full size regenerative air dustless sweeping technology sweeper; auxiliary engine: Deere 4045 FT4 turbocharged diesel, 99 hp;  hopper: 6 cu. yds.; water tank: 220 gallons; standard sweep path, max: 142\""]
["BI06","Tymco","Model 600: regenerative air sweeper; auxiliary engine: Deere 4045 FT4 turbocharged diesel , 99 hp; hopper: 7.3 cu.yds.; water tank: 220 gallons; standard sweep path, max: 142\""]
["BI07","Tymco","Model 500-X: high side dump regenerative air sweeper; auxiliary engine: Deere 4045 FT4 turbocharged diesel, 115 hp; hopper: 5.7 cu. yds., stainless steel; water tank: 250-gallons; dump height: 2-11'; standard sweep path, max: 142\" "]
["BJ01","Wayne","Gladiator: mechanical sweeper; auxiliary engine: Kuboda 3.6L diesel, 78 Hp; hopper: 5 cu yd, variable height; water tank: 340 gallons; standard sweep path: 144\""]
["BJ02","Wayne","Warrior: mechanical sweeper; single engine (chassis)design; hopper: 7 cu yds, variable hieght dump; water tank: 300 gallons; standard sweep path: 144\""]
["BJ03","Wayne","Warrior (CNG): mechanical sweeper; single engine (chassis) design; hopper 5.9 cu yds, variable hieght dump; water tank: 300 gallons; standard sweep parth: 144\" "]
["BJ04","Wayne","Centurion: mechanical, waterless-dustless sweeper; single engine (chassis) design; hopper: 6.8 cu yds, variable height dump; water tank: 300 gallons; dust control skirts, fan & filter; standard sweep path: 126\""]
["C: Airport Runway Sweepers"]
["CA01","Elgin","Crosswind FSX: recirculating air sweeper; auxiliary engine: Deere 4045TF diesel, 74 hp (EPA tier 4f); hopper: 8 cu.yds; water tank: 240 gallons; standard sweep path, max: 144\" (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["CB01","Johnston","VS801: vacuum sweeper; single engine design; gearbox auxiliary drive hydraulic drive system; hopper: 10.8 cu yds; water tank: 535 gallons; dual steering; standard sweep path, max: 144\""]
["CB02","Johnston","RT655R: regenerative air sweeper; auxiliary engine: Deere 4045HF, 115 hp; hopper: 8.5 cu. yds.; water tank: 250 gallons; dual broom; standard sweep path, max: 144”"]
["CC01","Schwarze","A7 Zephyr: regenerative air sweeper; auxiliary engine: Deere 4045T Tier IV Final  diesel, 115 hp; hopper: 8.4 cu. yds.; water tank: 250 gallons; standard sweep path, max: 144”"]
["CD01","Tymco","HSP: regenerative air high speed performance runway sweeper; auxiliary engine: Deere 4045T turbocharged diesel, 99 hp; hopper: 7.3 cu.yds.; water tank: 220 gallons; standard sweep path, max: 120\""]
["D: Commercial/Industrial Sweepers and Scrubbers - Walk-Behind Design   "]
["DA01","Advance (Nilfisk, Inc.)","7765 Propane (industrial series): sweeper-scrubber; 86 hp GM 3.0L; hopper: 16 cu. ft.; solution tank: 100 gallons; recovery tank: 100 gallons; standard scrub / sweep path: 54\" / 60\" "]
["DA02","Advance (Nilfisk, Inc.)","CS7000 (industrial series): sweeper-scrubber, hybrid propane / battery; hopper: 7 cu. ft., high dump; solution tank: 75 gallons; recovery tank: 75 gallons; standard scrub / sweep path: 48\" / 61\" "]
["DA03","Advance (Nilfisk, Inc.)","Adfinity (industrial series): scrubber; battery powered; solution tank: 14 gallons; recovery tank: 14 gallons; standard scrub path: 20\", disc pad "]
["DA04","Advance (Nilfisk, Inc.)","SC750 (industrial series): scrubber; battery powered; regular-to-heavy scrub applications; solution tank: 21 gallons; recovery tank: 21 gallons; standard scrub path: 26\", disc pad"]
["DA05","Advance (Nilfisk, Inc.)","SC800 (industrial series): scrubber; battery powered; regular-to-heavy scrub applications; solution tank: 25 gallons; recovery tank: 25 gallons; standard scrub path: 26\", disc pad"]
["DA06","Advance (Nilfisk, Inc.)","Warrior (industrial series): scrubber; battery powered; regular-to-heavy scrub applications; solution tank: 30 gallons; recovery tank: 30 gallons. standard scrub path: 28\", disc pad"]
["DA07","Advance (Nilfisk, Inc.)","Terra 28-B (commercial series): sweeper; battery powered; removable rider design: hopper: 2.1 cu. ft.; standard sweep path: 28\" "]
["DA08","Advance (Nilfisk, Inc.)","SW900 (commercial series): sweeper; battery powered; hopper: 1.8 cu. ft; standard sweep path: 32\""]
["DA09","Advance (Nilfisk, Inc.)","CFP polishers (commercial series): cleaner-polisher; power cord design; pad/brush: standard scrub path: 20\", disc pad"]
["DB01","Clarke (Nilfisk, Inc.)","Vantage 14: scrubber; battery powered; solution-recovery tank: 3 gallons; 14\" scrub path; 14\" disc pad"]
["DB02","Clarke (Nilfisk, Inc.)","CA90 32T: scrubber; battery powered; solution-recovery tank: 30 gallon/28 gallon; 32\" scrub path; 32\" disc pad"]
["DB03","Clarke (Nilfisk, Inc.)","Focus II MidSize: scrubber; battery powered; solution-recovery tank: 23 gallons; standard scrub path: 26\", disc pad"]
["DB04","Clarke (Nilfisk, Inc.)","Focus II MidSize BOOST: orbital technology for chemical free removal of floor finishes and scrubber; battery powered; solution-recovery tank: 23 gallons; standard scrub path: 28\" "]
["DB05","Clarke (Nilfisk, Inc.)","Focus II Compact: scrubber; battery powered; solution-recovery tank: 14.5 gallons; standard scrub path 20\", disc pad"]
["DB06","Clarke (Nilfisk, Inc.)","Focus II Compact BOOST: orbital technology for chemical free removal of floor finishes and scrubber; battery powered; solution-recovery tank: 14.5 gallons; standard scrub path: 20\" "]
["DB07","Clarke (Nilfisk, Inc.)","MA50 15B: scrubber; battery powered; solution-recovery tank: 3.5 gallons; 15\" scrub path; 15\" brush"]
["DB08","Clarke (Nilfisk, Inc.)","CA30 17E: scrubber; cord electric; solution-recovery tank: 13.2 gallons; 17\" scrub path; pad assist; 65 ft cord"]
["DB09","Clarke (Nilfisk, Inc.)","CA30 20B: scrubber; battery powered; solution-recovery tank 10.5 gallon; 20\" scrub path; pad holder"]
["DB10","Clarke (Nilfisk, Inc.)","FM 40 (commercial series): orbital floor cleaner-polisher; power cord design; pad / brush: 14\" x 20\" pad; solution tank: 2.5-gallons"]
["DB11","Clarke (Nilfisk, Inc.)","UltraSpeed Burnisher (commercial series): burnisher; power cord design; pad: 20\""]
["DB12","Clarke (Nilfisk, Inc.)","Ultraspeed 20 (commercial series): burnisher; battery powered; pad: standard path 20\" "]
["DB13","Clarke (Nilfisk, Inc.)","PBU Burnisher (commercial series): burnisher; propane powered; 603cc Kawasaki engine.  "]
["DD01","Minuteman","Kleen Sweep 27 - Collector 26 Battery Operated Sweeper:  26\" sweeping path; side broom; 1.4 cu. ft. hopper"]
["DD02","Minuteman","Collector 34B Battery Operated Sweeper:  34.25\" sweep path; 1.77 cu. ft. hopper; variable forward drive; on-board charger"]
["DD03","Minuteman","Phoenix 20 TD - Battery Operated Scrubber, Cylindrical: 20\" scrub path; 3.6 hp motor; medium duty brush. 12 gal. sol. tank. 13 gal. rec. tank. 3/4 hp vac motor; on-board charger"]
["DD04","Minuteman","Phoenix 24 Battery Operated Scrubber: trac drive; 24\" scrub path;   28\" squeegee; twin cylindrical brushes, medium duty; 19 gal.  sol. tank; 19.5 gal. rec. tank"]
["DD05","Minuteman","Phoenix 26 Battery Operted Scrubber: trac drive; 26\" scrub path; 37.4\" squeegee; twin disc brushes; 19 gal. sol. tank; 19 gal. rec. tank; 3/4 hp vacuum motor"]
["DD06","Minuteman","Phoenix 2830 Battery Operated Auto Scrubber - Cylindrical: 28\" scrub path;  37.4\" squeegee.  2-1 hp brush motors; twin brush pressure settings; 30 gal. sol. tank; 30 gal. rec. tank; 3/4 hp vacuum motor"]
["DD07","Minuteman","Phoenix 3330 Battery Operated Scrubber - Disc:  33\" scrub path; 43.3\" squeegee; twin disc brushes; 2-1 hp brush motors;  twin brush pressure settings; 30 gal. sol. tank; 30 gal. rec. tank; on-board charger; 3/4 hp vacuum motor"]
["E: Commercial/Industrial Sweeper - Riding Design"]
["EA01","Advance (Nilfisk, Inc.)","Proterra, propane (industrial series): sweeper; engine: Kubota, 31 hp; hopper: 11 cu. ft; standard sweep path: 51\" "]
["EA02","Advance (Nilfisk, Inc.)","SW8000: 4 Cylinder - Propane (industrial series): sweeper; engine: Kubota 4-cylinder gas, 57 hp; hopper: 14 cu. ft; standard sweep path: 65\" "]
["EA03","Advance (Nilfisk, Inc.)","SC6500 (industrial series): scrubber; battery powered; solution tank: 70 gallons; recovery tank: 70 gallons; standard scrub path: 40\""]
["EA04","Advance (Nilfisk, Inc.)","SC8000 (industrial series): scrubber; engine: 55 hp Kubota 1.6L propane; solution tank: 100 gallons; recovery tank: 100 gallons; standard scrub path: 48\""]
["EA05","Advance (Nilfisk, Inc.)","SW4000 (commercial series): sweeper; battery powered; hopper: 1.7 cu.ft.; standard sweep path: 37”"]
["EA06","Advance (Nilfisk, Inc.)","Adgressor 3220 (commercial series): scrubber; battery powered; solution tank: 42 gallons;  recovery tank: 42 gallons; standard scrub path: 32\""]
["EA07","Advance (Nilfisk, Inc.)","Advolution 2710 (commercial series): burnisher; battery powered; standard burnishing path: 27\""]
["EA08","Advance (Nilfisk, Inc.)","Advenger 2805D (commercial series): scrubber; battery powered; solution tank: 28 gallons;  recovery tank: 28 gallons; standard scrub path: 28\""]
["EB01","Clarke (Nilfisk, Inc.)","Focus II Rider: scrubber; battery powered; 30 gallon solution / recovery tank; scrub path: 28\""]
["EB02","Clarke (Nilfisk, Inc.)","Focus II Rider BOOST: orbital technology for chemical free removal of floor finishes and scrubber; battery powered; 30 gallon solution / recovery tank; scrub path: 32\""]
["EB03","Clarke (Nilfisk, Inc.)","MicroRider BOOST: orbital technology for chemical free removal of floor finishes and scrubber; battery powered; 21 gallon solution / recovery tank; standard scrub path: 28\" "]
["ED01","Minuteman","Admiral 28 Battery Operated Scrubber: 38\" squeegee; 30.6 gallon solution tank; 30 gallon recovery tank; 3/4 hp vacuum motor; standard scrub path: 28\""]
["ED02","Minuteman","Admiral 35 Battery Operated Scrubber: 38\" squeegee;  3/4 hp vacuum motor;  2x1 hp brush motor; 1 hp drive motor; 36.4 gallon solution tank; 36.4 gallon recovery tank; standard scrub path: 35\""]
["ED03","Minuteman","Admiral 40 Battery Operated Sweeper/Scrubber: 40\" scrub path; 2x 20\" brush discs; dust control; 50\" squeegee; 82 gallon solution tank; 82 gallon recovery tank; 0.82 hp vacuum motor;  standard sweep path: 55\""]
["ED04","Minuteman","APEX 47 Low Dump - Battery Operated Sweeper: 18\" side broom;  2.1 cu. ft. hopper; 60\" multi-level high dump; standard sweep path: 47\""]
["ED05","Minuteman","APEX 58 Sweeper Battery Operated Sweeper: single side broom; 31.5\" main broom. 4.6 cu ft hopper; 60\" high dump; standard sweep path: 45\""]
["ED06","Minuteman","Monitor 82 Manual Dump LP Powered Sweeper/Scrubber: 55 hp Kubota; 42\" sweep path; 42\" main broom; 5 cu. ft. hopper; 68 gallon solution tank; 65 gallon recovery tank; standard scrub path: 42\""]
["ED07","Minuteman","Monitor 90 Manual LP Powered Sweeper/Scrubber:  55 hp Kubota; 48\" sweep path; 48\" main broom; 6 cu. ft. hopper; 3 - 16\" disc brushes; 100 gal. sol. tank; 100 gal. rec. tank; standard scrub path: 48\""]
["ED08","Minuteman","Armadillo Gas Operated Sweeper - 6X: Kubota 23 hp; 36\" main broom; 24\" side broom; 10 cu. ft. hopper; 60\" high dump; 650 lb. hopper capacity: standard sweep path: 53\""]
["ED09","Minuteman","Armadillo Gas Operated Sweeper - 9X: 57 hp Kubota; 48\" main broom; 26\" side broom; 22 cu. ft. hopper; 64\" high dump;  1,500 lb. hopper capacity; standard sweep path: 64\""]
["ED10","Minuteman","Armadillo Gas Operated Sweeper - 10X:  57 hp Kubota; 56\" main broom; 26\" side broom; 30 cu. ft. hopper; 64\" high dump;  2000 lb. hopper capacity: standard sweep path: 74\""]
["ED11","Minuteman","Commander Gas Operated Scrubber/Sweeper - C82; 57 hp Kubota; 42\" main broom. 50\" squeegee; 68 gallon solution tank; 65 gallon recovery tank;  5 cu. ft. hopper; 250 lb. hopper capacity: standard sweep & scrub path: 42\""]
["ED12","Minuteman","Commander Gas Operated Scrubber/Sweeper - T82; 57 hp Kubota; 42\" main broom. 50\" squeegee; 68 gallon solution tank; 65 gallon recovery tank; 14 cu. ft. hopper; 1000 lb. hopper capacity: standard sweep & scrub path: 42\" "]
["ED13","Minuteman","Commander Gas Operated Scrubber / Sweeper - T90: 57 hp Kubota; 50\" squeegee; 100 gallon solution tank; 100 gallon recovery tank; 60\" multi-level high dump; 16 cu. ft., 1200 lb capacity hopper; standard sweep & scrub path: 50\""]
["ED14","Minuteman","Nautilus Gas Operated Scrubber  - P45GAS: 55 hp Kubota Gas; 50\" Cylindrical scrub path; 56\" squeegee; 105 gallon solution tank; 105 gallon recovery tank; manual dump; 2.1 cu. ft., 200 lb capacity  hopper "]
["ED15","Minuteman","Atlas Heavy Duty Sweeper - Pb620Dsl: 55 hp Tier III Kubota diesel; 1200 lb. hopper capacity; standard sweep path: 64\" (single side broom); hopper fire warning sensor"]
["F: Miscellaneous: Parking Lot, Walkway, Light Street, and Similar Applications"]
["FA01","Advance (Nilfisk, Inc.)","Cyclone CY5000: high pressure surface cleaner (purpose-built chassis design); built-in recovery; cab: enclosed with heat and AC; engine: Kubota turbo diesel, 66 hp; water tank: 360 gallons; cleaning path: 33\""]
["FA02","Advance (Nilfisk, Inc.)","Cyclone TR5000: high pressure surface cleaner (trailer-mounted dsign); engine: Kohler Command Pro gas,  27 hp; water tank: 360 gallons; cleaning path: 18\""]
["FA03","Advance (Nilfisk, Inc.)","Cyclone 4006AC: ultra high pressure rubber and marking removal system (purpose built chassis design); Built-in recovery; Cab: enclosed, wide cab design, heat and AC; Engine: 9.0L, 375 hp turbo diesel; Water Tank: 1600 gallons; cleaning path: 33\""]
["FA04","Advance (Nilfisk, Inc.)","Cyclone 4006ST: ultra high pressure rubber and marking removal system (commercial chassis design); built-in recovery; water tank: 530 gallons; cleaning path: 33\" (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["FA05","Advance (Nilfisk, Inc.)","Cylcone 4006LT: ultra high pressure rubber and marking removal system (commercial chassis design); built in recovery; water tank: 800 gallons; cleaning path: 33\"  (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["FA06","Advance (Nilfisk, Inc.)","Cyclone 4006HT: ultra high pressure rubber and marking removal system (commercial chassis design); built in recovery; water tank: 1600 gallons; cleaning path: 33\"  (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["FC01","Nite-Hawk","Osprey: vacuum sweeper; light truck chassis applications; single engine-PTO-hydraulic pump design; hopper: 2 cu. yds.; water tank: 30-gallons; standard sweep path, max: 81” (Offeror shall price their mandatory GM or Ford cab-chassis separately, on Form-E)"]
["FD01","Schwarze","Aero: parking lot sweeper; small pickup slip-in-mounting application; auxiliary engine: Robin EH65, gasoline, 22 hp; hopper: 2 cu. yds., rear manual unloading; water tank: 25 gallons; standard sweep path, max: 78\""]
["FE01","Schwarze","Aero - Trailer-Mount: parking lot sweeper; auxiliary engine:  Robin EH65, gasoline, 22 hp; hopper: 2 cu. yds., rear manual unloading; water tank: 25-gallons; standard sweep path, max: 78\""]
["FF01","Wayne","Vanguard: skid-steer mounted front broom; forward reach: 90\"; left side reach: 48\"; right side reach: 60\"  "]
["FG01","Waterblasting Technologies","SH7500 Stripe Hog: commercial chassis configuration; high pressure rubber and marking removal system with vacuum recovery; 40K psi @ 9 gallons per minute; Water tank: 1220 gallons; Maximum cleaning path: 36\" (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["FG02","Waterblasting Technologies","SH8000 Stripe Hog: commercial chassis configuration; high pressure rubber and marking removal system with vacuum recovery; 40K psi @ 12 gallons per minute; Water tank: 3150 gallons; maximum cleaning path: 72\" (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]
["FG03","Waterblasting Technologies","SK2000 Stripe Hog: skid configuration; high pressure rubber and marking removal system with vacuum recovery; 40K psi @ 5 gallons per minute; Water tank: 600 gallons; maximum cleaning path: 22\" (As per Section-B, Offeror shall price the body on this form, and may price optional chassis on Form-E)"]
["FG04","Waterblasting Technologies","SK3000 Stripe Hog: skid configuration; high pressure rubber and marking removal system with vacuum recovery; 40K psi @ 6 gallons per minute; Water tank: 1050 gallons; maximum cleaning path: 22\"  (As per Section-B, Offeror shall price the body on this form, and may price optional chassis on Form-E)"]
["FG05","Waterblasting Technologies","Surface Hog Surface Cleaner: commercial chassis configuration; high pressure surface cleaner with vacuum recovery; Water tank: 600 gallons; maxium cleaning path: 38\" (As per Section-B, Offeror shall price the body on this form, inclusive of mounting, and the mandatory factory-installed chassis on Form-E, noting accordingly)"]

{"sheet":"Form E","index":5,"n_rows":12,"n_cols":5,"rows_kept":12,"cut":false,"hidden":false,"merged":[[0,0,0,3],[3,0,3,4],[9,0,9,4],[1,1,1,4],[2,0,2,4],[10,0,10,4],[7,0,7,4],[6,0,6,4],[5,0,5,4],[4,0,4,4]]}
["FORM-E:  Options Pricing                                                                                        Invitation No.:",null,null,null,"SW04-16"]
["Offeror Name:"]
["*** Offerer should reference this Invitation's Section-B, subsection 6.0 and 7.0  ***"]
["(1) Bid each option item on a single, separate line. "]
["(2) Insert additional lines as necessary. A single (continuous) Form-E shall be used to price options for all models bid. "]
["(3) No handwritten entries"]
["(4) When pricing complete model upgrades on this form, such options shall be priced at the differential amount between associated Base Unit model's Form-D price and the optional (upgrade / downgrade) option. "]
["(5) All options priced herein must have a unique chassis manufacturer product / part code."]
["HGAC LINE ITEM PRODUCT CODE ASSSOCIATED WITH OPTION (e.g. \"AA01\", \"BA01-BA15\", \"All\", etc.)","OPTION NAME ","MANUFACTURER OPTION CODE","OPTION DESCRIPTION","H-GAC   PRICE, IN WHOLE DOLLARS"]
["NOTE: ALL priced manufacturer options must include a factory-to-dealer option code. Options that do not include such a parts code (or other data called for on this form) may be excluded from an awarded contract. Additionally, failure to include a comprehensive list of priced manufacture options may result in a non-compliant assessment for a given model, or overall"]
["Example"]
["AA01 - AA10","33\" broom upgrade","ABC-123","Larger curb side broom; brand: United"]

{"sheet":"W-9","index":6,"n_rows":3,"n_cols":1,"rows_kept":3,"cut":false,"hidden":false,"merged":[[2,0,2,10]]}
["W-9"]
[]
["Respondent should reference the W-9 form included in this solicitation package. It is a writeable form and should be completed and submitted with response in both printed and digital formats."]